Sentis-ToF-M100 API 1.0.0 API_for_using_the_Bluetechnix_Sentis_ToF_M100_camera

- Main Page
- Modules
- Data Structures
- Files

All Data Structures Files Functions Variables Typedefs Macros Groups Pages
Macros
Flags macros

API Flags. More...

## Macros
#define | HOLD_CONTROL_ALIVE 0x00000001
#define | SENTIS_NON_BLOCKING_INPUT 0x00000001

## Detailed Description

API Flags.

The following macros define the values of the flags that can be use in the API functions

## Macro Definition Documentation

#define HOLD_CONTROL_ALIVE 0x00000001

Indicate that the control connection will be opened until the handle is closed.

#define SENTIS_NON_BLOCKING_INPUT 0x00000001

Indicate that the STSgetData function should return without waiting if the frame queue is empty.