Sentis-ToF-M100 API 1.0.0 API_for_using_the_Bluetechnix_Sentis_ToF_M100_camera

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Macros Groups Pages
Functions
register.cpp File Reference
`#include <stdlib.h>`
`#include <stdio.h>`
`#include <m100api.h>`
Include dependency graph for register.cpp:

## Functions
int | main (int argc, char *argv[])

## Detailed Description

Version
  1.0.0

## Function Documentation

int main | ( | int | argc,
|  | char * | argv[]
| ) |  |

# DESCRIPTION

Example application for the sentis-ToF-m100 camera API

This application shows how to connect to the camera with the default network values and how to read the registers.

It reads all the status registers of the camera and prints the values in the console.