Sentis-ToF-M100 API 1.0.0 API_for_using_the_Bluetechnix_Sentis_ToF_M100_camera

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

- All
- Variables

All Data Structures Files Functions Variables Typedefs Macros Groups Pages
Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

- bytesPerPixel : T_SENTIS_DATA_HEADER
- firmwareVersion : T_SENTIS_DATA_HEADER
- flags : T_SENTIS_CONFIG
- frameCounter : T_SENTIS_DATA_HEADER
- headerCrc16 : T_SENTIS_DATA_HEADER
- headerVersion : T_SENTIS_DATA_HEADER
- imageFormat : T_SENTIS_DATA_HEADER
- imageHeight : T_SENTIS_DATA_HEADER
- imageWidth : T_SENTIS_DATA_HEADER
- ledTemp : T_SENTIS_DATA_HEADER
- mainTemp : T_SENTIS_DATA_HEADER
- nofChannels : T_SENTIS_DATA_HEADER
- reserved1 : T_SENTIS_DATA_HEADER
- reserved2 : T_SENTIS_DATA_HEADER
- reserved3 : T_SENTIS_DATA_HEADER
- tcp_ip : T_SENTIS_CONFIG
- tcp_port : T_SENTIS_CONFIG
- timestamp : T_SENTIS_DATA_HEADER
- udp_ip : T_SENTIS_CONFIG
- udp_port : T_SENTIS_CONFIG