Sentis-ToF-M100 API 1.0.0 API_for_using_the_Bluetechnix_Sentis_ToF_M100_camera

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Macros Groups Pages
Data Fields
T_SENTIS_CONFIG Struct Reference

Configuration structure. More...

`#include <apitypes.h>`

## Data Fields
unsigned short | udp_port
unsigned short | tcp_port
unsigned | flags
char const * | tcp_ip
char const * | udp_ip

## Detailed Description

Configuration structure.

This structure is used for configuring the API and for setting the connection parameters. It is used in the STSOpen function

## Field Documentation

unsigned T_SENTIS_CONFIG::flags

Bit level set unsigned for flags. Used for forcing a specific behavior of the connection.

char const* T_SENTIS_CONFIG::tcp_ip

Pointer to the string with the tcp ip address in network pointed format.

unsigned short T_SENTIS_CONFIG::tcp_port

The tcp port to use.

char const* T_SENTIS_CONFIG::udp_ip

Pointer to the string with the udp multicast group ip address in network pointed format.

unsigned short T_SENTIS_CONFIG::udp_port

The udp port to use.

The documentation for this struct was generated from the following file:

- include/apitypes.h