The main differencies between the single versions are the supported peripherals.
The "standalone" versions doesnt support peripherals.

Because some of the peripherals are connected in different ways on different basis board versions,
we provide a binary for each basis board version. 

If there are no differencies we provide a single binary for all versions.

(c) Bluetechnix 2006
