# Design Rule Verification Report

Date: |  | 03.10.2018
Time: |  | 09:14:09
Elapsed Time: |  | 00:00:12
Filename: |  | T:\prjbluetechnix\Melexis\MLX75123-Eval\phase3_development\hardware\EVK75123-Sensor-MLX75024\layout\EVK75123-MLX75024.PcbDoc
Warnings: |  | 0
Rule Violations: |  | 0

## Summary

Warnings | Count
--- | ---
Total | 0

Rule Violations | Count
--- | ---
Clearance Constraint (Gap=0.4mm) (InPolygon),(InPadClass('MH')) | 0
Clearance Constraint (Gap=0.23mm) (All),(not PadIsPlated) | 0
Clearance Constraint (Gap=0.1mm) (All),(All) | 0
Short-Circuit Constraint (Allowed=No) (All),(All) | 0
Un-Routed Net Constraint ( (All) ) | 0
Modified Polygon (Allow modified: No), (Allow shelved: No) | 0
Width Constraint (Min=0.1mm) (Max=3mm) (Preferred=0.15mm) (All) | 0
Differential Pairs Uncoupled Length using the Gap Constraints (Min=0.1mm) (Max=0.1mm) (Prefered=0.1mm) and Width Constraints (Min=0.12mm) (Max=0.12mm) (Prefered=0.12mm) (InNetClass('DIFF100')) | 0
Differential Pairs Uncoupled Length using the Gap Constraints (Min=0.12mm) (Max=0.12mm) (Prefered=0.12mm) and Width Constraints (Min=0.1mm) (Max=0.1mm) (Prefered=0.1mm) (InDifferentialPair ('D')) | 0
Power Plane Connect Rule(Direct Connect )(Expansion=0.5mm) (Conductor Width=0.3mm) (Air Gap=0.2mm) (Entries=4) (All) | 0
Hole Size Constraint (Min=0.1mm) (Max=4mm) (All) | 0
Pads and Vias to follow the Drill pairs settings | 0
Hole To Hole Clearance (Gap=0.15mm) (All),(All) | 0
Minimum Solder Mask Sliver (Gap=0.1mm) (All),(IsVia) | 0
Net Antennae (Tolerance=0mm) (All) | 0
Matched Lengths(Tolerance=25.4mm) (InDifferentialPair ('DDR.CLK')) | 0
Vias Under SMD Constraint (Allowed=Allowed) (All) | 0
Height Constraint (Min=0mm) (Max=25.4mm) (Prefered=12.7mm) (All) | 0
Total | 0