The loader file FlashNewBS_CM-5xx.ldr contains a tool to flash a new BLACKSheep version overwriting the old one allready installed.
Use this file if for some reasons you cannot flash the coremodule with the flash command from the BLACKSheep console.

Select the correct file for your core module.

Install instructions:

-Type "xmr updatetool" on the BLACKSheep console.
-Transfer the file "FlashNewBS.ldr" using the filetransfer option of your terminal program. Use the xmodem protocol.
-Type "exec updatetool" on the BLACKSheep console.

The updatetool should start now. PLease follow the instructions printed out on the terminal.

Refer to the BLACKSheepCommandReference to learn more about the BLACKSheep commands.

(c) Bluetechnix 2006